Dow logo

Dow High Performance Building

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

DOWSIL™ 796 Neutral Silicone

A one-part, low modulus, neutral curing silicone sealant specifically developed for the sealing of PVC-U, glass, glazed surfaces and brickwork

* Good unprimed adhesion to a variety of substrates
* Low modulus, high elasticity
* 100% silicone sealant
* Conforms to ISO 11600-F&G-25LM, SNJF Vitrage et Façade Category 1, EN 15651 - CE MARK
* Resistant to ozone, ultra-violet radiation and temperature extremes

|  |  |
| --- | --- |
| WhiteWarm WhiteAnthrazite  |  |
| Black  |  |
| Bronze  |  |
| Brown  |  |
| French Limestone  |  |
| Gold Oak  |  |
| Grey  |  |
| Marron Wood  |  |
| Boston Grey  |  |
| RAL 7016 |  |
|  |  |

This color card is only intended for reference use.

Please contact your local Dow sales office or Dow distributor for more information about availability, packaging, lead times and prices.

Custom colors may be available upon request.

**For more information**

Learn more about Dow’s full range of High Performance Building solutions, including service and support at [www.dow.com/construction](http://www.dow.com/construction).

Dow has sales offices, manufacturing sites and science and technology laboratories around the globe. Find local contact information at [www.dow.com/ContactUs](http://www.dow.com/ContactUs).



Eckart: please can you change 2018 to 2019 below and remove S88775/E88679 reference. I have requested a new form number and will send along soon

